; The following is an example AP_CFG.TXT file. Make changes to this file
; to match your site-specific network settings.


[APInstallation]
;UnitName              testhost.intel.com     ;up to 31 chars
;IPAddress             157.235.101.33         ;comment out if DHCP enabled
Gateway1               157.235.101.1
Gateway2               157.235.101.2
SubNetMask             255.255.255.0
NetID                  Engineering            ;up to 32 chars
AntennaSelect          Primary Only           ;"Full Diversity"
                                              ;"Primary Only"
                                              ;"Secondary Only"
                                              ;"Rx Diversity"
DHCP                   Enabled                ; "Disabled"
                                              ; "Enabled"
                                              ; "DHCP Only"
                                              ; "BOOTP Only"
DNSServer1             157.235.101.1
DNSServer2             157.235.101.2
DNSServer3             157.235.101.3


[SpecialFunction]
FWFileName             intl3_fw.bin           ;up to 30 chars
HTMLFileName           intl3_htm.bin          ;up to 30 chars
ConfigFileName         ap_cfg.txt             ;up to 30 chars ***New***
ACLFileName            ap_acl.txt             ;up to 30 chars ***New***
;HelpURL               www.intel.com          ;up to 30 chars
TFTPServer             tftp.apfw.intel.com    ;ip address or name


[SystemConfig]
Channel                2                      ; 1 - 11 
AutoChannelSelect      Disabled               ; "Disabled", "Enabled"
EthernetTimeOut        0                      ; 0: disabled,
                                              ; 1: hw detection,
                                              ; 2,3,4: WLAP detection,
                                              ; 30 - 255 seconds: sw detection
TelnetLogins           Enabled                ; "Disabled", "Enabled"
AgentAdInterval        0                      ; 0 - 1200 seconds
S24MobileIP            Disabled               ; "Disabled", "Enabled"
MobileHomeMD5Key       Intel                  ; up to 13 chars
InternationalMode      Disabled               ; "Disabled", "Enabled"
WebServer              Enabled                ; "Disabled", "Enabled"
AccessControl          Disabled               ; "Disabled", "Allowed", "Disallowed"
TypeFiltering          Disabled               ; "Disabled", "Forward", "Discard"
WNMPFunctions          Enabled                ; "Disabled", "Enabled"
APAPStateExchange      Enabled                ; "Disabled", "Enabled", "1", "4"
TypeFiltering          Disabled               ; "Disabled", "Forward", "Discard"
WNMPFunctions          Enabled                ; "Disabled", "Enabled"
APAPStateExchange      Enabled                ; "Disabled", "Enabled", "1", "4"
EthernetInterface      On                     ; "Off", "On"
RFInterface            On                     ; "Off", "On"
DefaultInterface       Ethernet               ; "Ethernet",
MUMUDisallowed         Off                    ; "Off", "On"
;AdminPassword         Intel                  ; up to 13 chars
;UserPassword          Intel                  ; up to 13 chars
InactivityTimeout      5                      ; 0 - 9999
ModemConnected         No                     ; "No", "Yes"
Kerberos               Disabled               ; "Disabled", "Enabled"
KDCName                krbtgt                 ; up to 128 chars
KSSName                ksssrv                 ; up to 128 chars
KSSPort                34567                  : 0 - 99999
RealmName              apfw.intel.com         ; up to 128 chars
KerberosUserID         KerberosTest           ; up to 32 chars
KerberosPassword       Intel                  ; up to 32 chars
TimeZone               PST                    ; GMT, BST, IST, WET, WEST,
                                              ; CET, CEST, EET, EEST, MSK,
                                              ; MSD, AST, ADT, EST, EDT,
                                              ; CST, CDT, MST, MDT, PST,
                                              ; PDT, HST, AKST, AKDT, WST
ClockSkew              300                    ; 0 - 99999


[RFConfig]
DTIMInterval           10                     ; 1- 255
BCMCQMax               100                    ; 0 - 100
ReassemblyTimeout      9000                   ; 0 - 9999
MaxRetriesData         15                     ; 0 - 32
MaxRetriesVoice        5                      ; 0 - 32
MulticastMaskData      09000E00
MulticastMaskVoice     01005E00
BeaconInterval         100                    ; 20 - 1000
AcceptBroadcastESSID   Disabled               ; "Disabled", "Enabled"
MUInactivityTimeout    60                     ; 3 - 600
TransmitRate1          Required               ; "NotUsed", "Optional", "Required"
TransmitRate2          Required               ; "NotUsed", "Optional", "Required"
TransmitRate5.5        Optional               ; "NotUsed", "Optional", "Required"
TransmitRate11         Optional               ; "NotUsed", "Optional", "Required"
FragmentationThreshold 572                    ; 256 - 2346
RTSThreshold           100                    ; 0 - 2347
WLAPMode               Disabled               ; "Disabled",
                                              ; "Enabled",
                                              ; "LinkRequired"
WLAPPriority           8000                   ; 0 - FFFF
WLAPManualBSSID        00:A0:F8:00:B8:B9
WLAPHelloTime          20                     ; 0 - 9999
WLAPMaxAge             100                    ; 0 - 9999
WLAPForwardDelay       5                      ; 0 - 9999
WEPPrivacy             Disabled               ; "Disabled", "Enabled"
WEPAlgorithm           40BitSharedKey         ; 40BitSharedKey
                                              ; 128BitSharedkey"
EncryptionKeyID        1                      ;  1 - 4 
EncryptionKey1         1011121314
EncryptionKey2         2021222324
EncryptionKey3         3031323334
EncryptionKey4         4041424344
TxPowerControl         Full                   ; "Full", "30mW", "15mW", "5mW", "1mW"


[SNMPConfig]
AgentMode              ReadOnly               ; "Disable",
                                              ; "ReadOnly",
                                              ; "ReadWrite"
TrapHost1              157.235.101.101        ; ip address or name
TrapHost2              157.235.101.102        ; ip address or name
ReadOnlyCommunity      public                 ; up to 31 chars
ReadWriteCommunity     admin                  ; up to 13 chars 
AllTraps               Enabled                ; "Disabled", "Enabled"
ColdBoot               TrapHost2Only          ; "Disabled",
                                              ; "TrapHost1Only"
                                              ; "TrapHost2Only"
                                              ; "AllTrapHosts"
AuthenticationFailure  TrapHost1Only          ; "Disabled",
                                              ; "TrapHost1Only"
                                              ; "TrapHost2Only"
                                              ; "AllTrapHosts"
RadioRestart           TrapHost2Only          ; "Disabled",
                                              ; "TrapHost1Only"
                                              ; "TrapHost2Only"
                                              ; "AllTrapHosts"
AccessViolation        AllTrapHosts           ; "Disabled",
                                              ; "TrapHost1Only"
                                              ; "TrapHost2Only"
                                              ; "AllTrapHosts"
MUStateChange          TrapHost1Only          ; "Disabled",
                                              ; "TrapHost1Only"
                                              ; "TrapHost2Only"
                                              ; "AllTrapHosts"
WLAPConnectionChange   TrapHost2Only          ; "Disabled",
                                              ; "TrapHost1Only"
                                              ; "TrapHost2Only"
                                              ; "AllTrapHosts"
DHCPChange             AllTrapHosts           ; "Disabled",
                                              ; "TrapHost1Only"
                                              ; "TrapHost2Only"
                                              ; "AllTrapHosts"
KerberosError          TrapHost2Only          ; "Disabled",
                                              ; "TrapHost1Only"
                                              ; "TrapHost2Only"
                                              ; "AllTrapHosts"


[EventLogConfig]
AnyEventLogging        Enabled                ; "Disabled","Enabled"
SecurityViolation      Disabled               ; "Disabled","Enabled"
MUStateChanges         Enabled                ; "Disabled","Enabled"
WNMPEvents             Enabled                ; "Disabled","Enabled"
SerialPortEvents       Enabled                ; "Disabled","Enabled"
APAPMessages           Disabled               ; "Disabled","Enabled"
TelnetLogins           Enabled                ; "Disabled","Enabled"
SystemEvents           Enabled                ; "Disabled","Enabled"
EthernetEvents         Disabled               ; "Disabled","Enabled"
